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) 	Secure The World With You




















H.265+/H.265/H.264+/H.264/MJPEG coding
Max.resolution: 8MP ( 3840 × 2160 ) ICR auto switch, true day / night vision
3D DNR, true WDR, HLC, BLC, smart IR and ROI coding 30~50m IR night view distance
1CH audio input; 1CH built-in MIC Built-in micro SD card slot, up to 256GB DC12V/PoE power supply
Support three streams IP 67
Support mobile surveillance by smart phones with iOS and Android OS Intelligent analytics
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For more information, please visit our website




Shenzhen TVT DIGITAL TECHNOLOGY CO., LTD.
Address: 23rd Floor, Block B4, Building NO.9, Shenzhen Bay Eco-Technology Park, Nanshan District, Shenzhen, Guangdong Province, P.R.China



Tel: +86-755-36995888	Fax: +86-755-33104777
Web site: http://en.tvt.net.cn	E-mail: overseas@tvt.net.cn
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TD-9585S3B
Camera
8MP Turret Network
) (
Model
Specifications
TD-9585S3B
Camera
Image Sensor
1 / 2.8 "CMOS
Image Size
3840×2160
Electronic Shutter
1 / 2 s ~ 1 / 100000 s
Iris Type
DC Iris
Min
. 
Illumination
0.02 lux @ F1.6, AGC ON; 0 lux with IR
~
Lens
2.8 
12mm@F1.6,
 motorized
~
~
~
Field of View
Horizontal:99° 33°
; 
Vertical 
:
53° 17°
; 
Diagonal
:
117° 37°
Φ
Lens Mount
14
Day&Night
ICR
Wide Dynamic Range
120dB
BLC
Yes
HLC
Yes
Defog
Yes
Digital NR
3D DNR
S/N Ratio
≥
50dB
Angle Adjustment
Pan: 0
°
~360
°
; Tilt:0
°
~80
°; 
Rotation: 0
°
~360
°
DORI Distance
Lens
Detect
Observe
Recognize
Identify
2.8
~
12mm
(
W
)
86.65m(284.28ft)
34.66m(113.71ft)
17.33m(56.85ft)
8.66m(28.41ft)
2.8
~
12mm
(
T
)
289.06m(552.31ft)
115.62m(240.12ft)
57.81m(136.06ft)
28.91m(84.04ft)
Image
Video Compression
Main stream
: 
H.265+ / H.265 / H.264+ / H.264
Sub 
stream
: 
H.265+ / H.265 / H.264+ / H.264 / MJPEG
Third 
stream
: 
H.265+ / H.265 / H.264+ / H.264 / MJPEG
H.264 Compression Standard
Baseline Profile/Main Profile/High Profile
Resolution
8MP ( 3840 × 2160 ), 6MP( 3072 × 2048 ),5MP( 2592 × 1944),
4MP ( 2592 × 1520), 2K(2560 × 1440 ), 3MP(2304 × 1296),
1080P ( 1920 × 1080 ), 720P ( 1280 × 720 ), D1, CIF, 480 × 240
Main Stream
60Hz
 
:
 
8MP(1~20fps)/6MP/5MP/4MP/2K/3MP/1080P/720P(1
~
30fps)
50Hz
 
:
 
8MP(1~20fps)/6MP/5MP/4MP/2K/3MP/1080P/720P(1
~
25fps)
Sub Stream
60Hz: 720P(1~12fps)/D1/480 × 240(1~30fps)
50Hz: 720P/D1/480 × 240(1~25fps)
Third Stream
60Hz:
 
720P/D1/CIF/480
 
×
 
240 
(1~30fps)
50Hz:
 
720P/D1/CIF/480
 
×
 
240 
(1~25fps)
Bit Rate
64 Kbps ~ 12 Mbps
Bit Rate Type
VBR / CBR
Audio Compression
G711A / U
Image Settings
ROI, Saturation, Brightness, Hue, Contrast, Wide Dynamic, image mirror, image flip, Sharpness, NR, etc. adjustable through client software or web browser
ROI
Each ROI to be configured separately
Interfaces
Network
RJ 45 10M/100M self
-
adaptive Ethernet port
Video Output
No
Audio
1CH built-in MIC; 1CH audio input
Alarm
No
Storage
Built-in micro SD card slot; up to 256GB
Reset
Yes
Functions
Remote Monitoring
IE browser/ TVT NVR / NVMS / mobile APP
Web Browser
IE11(plug-in required)/Chrome 89.0+/Edge 89.0+/Firefox 87.0+/Safari 14.0+
Online Connection
Support simultaneous monitoring for up to 10 users; Support multi-stream real time transmission
Network Protocol
UDP, IPv4, IPv6, DHCP, NTP, RTSP, RTP, RTMP, RTCP, PPPoE, DDNS, SMTP, FTP, SNMP, HTTP, HTTP POST, 802.1x, UPnP, HTTPs, QoS
Interface Protocol
ONVIF
Storage
Network remote storage; micro SD card storage
Smart Alarm
Motion detection; SD card error; SD card full
Intelligent Analytics
Scene change, video blur detection, abnormal color detection , line crossing detection, intrusion detection
)SPECIFICATIONS	




	General function
	Watermark, video mask, heartbeat,corridor pattern

	
Security
	Video encryption, firmware encryption, HTTPs encryption, configuration encryption, illegal login lock, IP address filtering, 802.1x authentication, basic and digest authentication for HTTP/HTTPs

	IR Distance
	30~50m

	Protection Grade
	IP 67

	PoE
	Yes (IEEE802.3af)

	Others

	Power Supply
	DC12V/PoE

	Power Consumption
	< 8W

	Storage Conditions
	- 30 °C ~ 65°C (-22°F~149°F), Humidity: less than 95 % (non-condensing)

	Operating Conditions
	- 30 °C ~ 60 °C (-22°F~140°F), Humidity: less than 95 % (non-condensing)
Φ

	Dimensions ( mm )
	111.5 × 99.6

	Weight ( net )
	Approx. 0.661KG

	Installation
	Ceiling mounting; Wall mounting

	Certificate
	CE, FCC

	Environmental Protection
	Complies with Directive EU RoHS, WEEE(2012/19/EU) , directive 94/62/EC and REACH(EC1907/2006)
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 AVAILABLE ACCESSORIES	

 (
TD-YXH0302+ TD-YZJ0811
TD-YXH0302+
TD-YZJ0407+TD-YZJ0601
TD-YXH0302+
TD-YZJ0407+TD-YZJ0501
TD-YZJ0203
TD-YXH0106
TD-YXH0302
)


AVAILABLE MODEL	

 (
en.tvt.net.cn
*All pictures and specifications are for reference only and are subject to change without prior notice.
)

 (
TD-9585S3B(D/AZ/PE/AR3)
Available Model
)
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